Installation:


1. Start Windows (3.1., 3.1.1. or Windows 95).

2. Put disk in drive a:.

3. Run a:\setup.exe and follow the instructions on screen.
 

--------------------- DISCLAIMER -----------------------------
     
VAASA CONTROL OY DISCLAIMS ALL WARRANTIES, EITHER EXPRESS OR IMPLIED,
INCLUDING, BUT NOT LIMITED TO IMPLIED WARRANTIES OF MERCHANTABILITY
AND FITNESS FOR A PARTICULAR PURPOSE, WITH RESPECT TO THE PRODUCT.
SHOULD THE PROGRAM PROVE DEFECTIVE, THE PURCHASER ASSUMES 
THE RISK OF PAYING THE ENTIRE COST OF ALL NECESSARY SERVICING, REPAIR,
OR CORRECTION AND ANY INCIDENTAL OR CONSEQUENTIAL DAMAGES.  
IN NO EVENT WILL VAASA CONTROL OY BE LIABLE FOR ANY DAMAGES WHATSOEVER
(INCLUDING WITHOUT LIMITATION DAMAGES FOR LOSS OF BUSINESS PROFITS, 
BUSINESS INTERRUPTION, LOSS OF BUSINESS INFORMATION AND THE LIKE) ARISING 
OUT OF THE USE OR THE INABILITY TO USE THIS PRODUCT EVEN IF VAASA CONTROL OY
HAS BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES. INSTALLING THE PROGRAM
INDICATES YOUR ACCEPTANCE OF THESE TERMS.
