==================================================================
LX-DSWSC AX Wizard,   3.4  ReadMe File,      August 27, 2012
Copyright (c) 2012 Johnson Controls Inc.  All Rights Reserved.
==================================================================

This package is the initial software of the Johnson Controls 
LX-DSWSC device Wizard. 

This software may configure LX-DSWSC devices in
EC-BOS AX platforms with EC-NET-AX support pack 2.5.0 or later.

The Johnson Controls AX Wizards are client/server applications that 
require software to be installed on EC-BOS AX platforms and on any 
client machine running the Wizards. This package is a client machine
installation.

This installation package comprises of the LX-DSWSC AX Wizard. 
Also included are the external interface file (XIF), the device 
application program (APB) and the device resource files (DRF) for 
using the LX-DSWSC device.

After Setup, the following software and file versions will be 
installed on your computer:

- Johnson Controls LX-DSWSC Wizard		    Version 3.4.xxx
- LonMark Standard Device Resource Files            Version 13.10
- Johnson Controls Device Resource Files (scope 3)  Version 1.21
- LX-DSWSC External Interface File		  LXDSWSC211.XIF
- LX-DSWSC Application Program		  LXDSWSC_v267.APB
- LX-DSWSC Application Program		  LXDSWSC_v267.NXE


!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!!!!!!!!!!!!!!!!!!!!!!!!! IMPORTANT NOTICE !!!!!!!!!!!!!!!!!!!!!!!!
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

Make sure you have installed EC-NET-AX v3.5.34 and support pack v3.2.x.xx to use the new ECL controllers.
If the ECL controllers are not planned to be used, there is no need to upgrade EC-NET-AX and support pack.

Installation of this Wizard breaks the compatibility 
with EC-BOS AX platforms loaded with Support Pack 2.2 or earlier.

Therefore before installing this Wizard, please make 
sure that this computer will not be required for the
configuration of any EC-BOS AX platforms with Support Pack 2.2 or
earlier.

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!


I. Client installation (integrator computer)
============================================

This installation procedure must be followed before using the LX-DSWSC 
AX Wizard. It is intended for any PC computer or laptop from which 
the LX-DSWSC AX Wizard will be used.

Requirements : PC / Windows 2000, 2003, XP, Vista, 7

1.  Close any running Wizard applications.
2.  Run the setup file: LX-DSWSC Configuration v3.4.xxx Setup.exe



II. Wizard initial running Instructions
=======================================

See the instructions in the EC-NET-AX support package.

III.I New Features and Problems Fixed (Firmwaire)
====================================

Version 2.67 (2011-04-29)
	- Modification : Try first the standard way to write into a network variable input and on response failed
                       try the extended command mode.

Version 2.66 (2011-04-13)
	- Bug fix : Display properly a standard network variable on a host based node (NV_index bigger than 254).
	- Feature : Modify a standard network variable by using the Extended Command Set described in the
                  ANSI/CEA-709.1-B document.
 
Version 2.65 (2011-04-04)
	- Bug fix : Read MSB first for bit field on the UNVT_variable_bool.

Version 2.64 (2011-03-11)
	- Feature : Support the ECL series.
             Mode and value for internal points are on the same line for ECL controllers
             and ECP controllers (gfx version only).
             For variable (float type) in write mode, NAN and -NAN values are available.

Version 2.62 (2008-07-22)
	- Modification : Increase memory size for the Display configuration file
	                 (used by the plug-in).
	- Modification : Support internal points of new gfx free programmable controllers.

Version 2.53 (20-6-2007)

	- Bug fix : Changed the default values for Daylight Savings Time.
	- Bug fix : Supported the 16 inputs of ECP-500.

Version 2.52 (19-10-2005)

	- Bug fix : In write mode (display section), now able to change a datapoint
                    at the upper and lower limits of its value.
	- Bug fix : In write mode (display section), rounded numbers to not lose somes steps.

Version 2.51 (20-01-2005)

	- Modification : Reduced the contrast to prevent character bleeding on the screen.
	- Modification : Changed device minor version from 5 to 51 to incorporate 2 digit versioning.

Version 2.5 (13-04-2004)

	- Modification : Added a general log off timeout.
	- Start with this version for changes.

   
III.II New Features and Problems fixed (Wizard)
====================================
Version 3.4
01. Supports ECL Series Dynamic Wireless and ComSensor internal points.

Version 3.3                                                              
01. Bug Fixed: Password page freezes.                                    
02: Bug Fixed: Data Point name was cut off to 13 letters.                
03: Bug Fixed: Internal point's write enable property was always on.    
04: Bug Fixed: Poll Interval was always 1 second. 

Version 3.2
01. Updated: Support ECL600 Device
02. Added: CRC32 checks: download is much more efficent.
03. Added: the enum name appears in the window of the selection data point if applicable
04. Updated: Enumeration magager:
	a) Copy/paste (multiple items);
	b) edit enumeration tool:  auto operations;
	c) display more infomation about enum like whether it is in use or not and it is editing or not.
	d) import enumeration from DRF.
05. Added: Support format (ex. SNVT_temp_p#Si, SNVT_Temp_p#US) on a type (ex. SNVT_temp_p) on Multiplier, Offset and unit.
06. Fixed: The plug-In crashed while loading a selected data point type of the SNVT_clothing_w_s.
07. Fixed: Couldn't selecting the field in a nv type if the type contains reference (ex. SNVT_clothing_w_s).
08. Fixed: The signature was never updated


Version 3.1.238
----------------
01. Fixed: Using network variable index as collection position.
02. Fixed: Couldn't use the network variable if its index was in [156, 171].
03. Fixed: The application couldn't show up to front after launching 

Version 3.0
----------------
01. Updated: The plug-In is much more productive and very user-friendly than ever.
	     More than 60% code re-wroted on OOP style. This makes the plug-In more efficient, more 
	     performent, much more stable and more flexible. 
	     for example, Loading plug-in is faster; connecting data point is faster in the tree view; 
	     Easy to connect multiple data points by copy/paste and change device (see below) or by Johnson Controls 
	     Browser; Easy to use user-defined enumeration, ...
02.   Added: Support LXPRGXXX gpi series.
03.   Added: (Second and third generation) internal point name is defined in DRF.
04.   Added: Listview interface of data points: All the data points are accessible in the listview.
05.   Added: Copy (Ctrl c),Cut (Ctrl x), Paste (Ctrl v), insert, clear (Ctrl l), delete (Del), undo (Ctrl z), 
	      select (Ctrl a) and deselect (Ctrl d) data points by popup menu and by Keyboard in listview.
	     All the above functions are standard like Excel.
	     Copied data can be used multiple times and user can also decide himself to delete them by clciking
	     the item "Clear copied/cut data points" in popup menu
06.   Added: Drag and drop data points to move (Drag and drop: Insert cut data point(s)) or copy 
	     (Ctrl + Drag and drop: Insert copied data point(s)).
07.   Added: Change linked device in data points.
08.   Added: 40 Undo levels for data points in listview.   
09. Changed: An enum will not removed automatically if there is some free space
10.   Added: Add and Remove internal Enums freely by user. In case that it needs to 
	     remove unused enum, the item will be chosen by FIFO.
11.   Added: Enumeration name: it is used only in database (not in controller) but saved also in controller. 
12.   Added: Allow user to rename enum member's name.
13.   Added: Allow user to add and remove enum member. Different colors are used in the internal enums listview. 
	     And blue  color means the item is in use, red color means not empty but not used and gray 
             color means the item is empty. Each item has a check box and only the red one can be selected (checked).
	     The delete button will be enabled when some item is checked and click the delete button the checked 
	     item will be deleted.
14.   Added: Allow user to create an enumeration himself.
15.   Added: Export and Import data points, enums and Logo with Xml file (the xml 
             files is compatible to LNS).
16.   Added: Progress bar window to start plug-in (standard).
17. Changed: Enumeration will not be listed if it marked as deleted item (a "~" in name).
18.   Added: Link broken if a data point cannot find the reference device via subnetid and nodeId: 
	     The item path text and list item device column are on red color and display subnet id 
	     and node id value and also device type (like ECP203 gfx) or device Program id if the 
	     device type is unknown and a valid program id saved for this point. Note that no program id was saved 
	     in the the database created by LX-DSWSC v2.6 or earlier or by lonwatcher 3.2.1346 or earlier.  
19. Changed: The list of enumerations sorts by alphabet on names.
20.   Added: Much more information will be displayed on message window and less hardcoded messages will appear.
21.   Fixed: Navigating in network treeview by double click on an object invoked an invalid object error. 
22.   Fixed: Plug-In crashed when loaded a drf enum with only one or more negative value members.
23.   Fixed: Plug-In crashed when no reference could be found on the subnet id and the node id.
24.   Fixed: Added real error description in message logger for the following bug: The error 
	     "Unable to modify location string" appeared without an evident reason.
  

IV. Known Problems and Workarounds
===================================

1.   In the "Item Selection" menu, the full interface consisting 
     of the Network Configuration Inputs ("NCIs") and Network 
     Variables ("NVOs" and "NVIs") is normally discoved for all 
     Lonworks Devices and the LocalLonDevice in the station, except 
     in the following cases :

     a) The Network configuration inputs ("NCIs") are not discovered 
        in devices when they are related to a Netowrk Variable 
        (i.e. their NcProps/Scope property equal "Nv").

     b) The Network Variables and Network Configuration Inputs 
        ("NVs" and "NCIs") may not be discovered for non interoperable 
        device (Program IDs not starting with "80" or "90").

     c) A one to one mapping between the Program ID and the lnml file 
        is assumed. The device interface may not be discovered properly
        if a device with a different interface and the same Program ID 
        was previously discoved (as this is the case for some non 
        interoperable devices of some manufacturers).

2.   The message "No DRF is available for this network variable" 
     in the Item Selection menu, indicates that DRF files are missing 
     in the client computer.

     When this situation occurs with devices from other manufacturers, 
     copy the DRF files specific to this device to a directory under 
     the "C:\LonWorks\Types\User\[...]" directory and use the 
     "LNS Resource File Catalog Utility"  to add the directory to the 
     DRF device catalog.
     
     If the latter application is not installed on the client computer, 
     use another computer with this application to generate the proper 
     catalog (C:\LonWorks\Types\ldrf.cat).

     To add the Johnson Controls FreeProgrammable or EC-Stat device 
     specific DRFs to the catalog, install the Wizards respective to 
     these devices and run the Wizards once (offline) to generate 
     the catalog.

3.   The ncis (Network Configuration Inputs) of scope 4 
     (ncProps/snvtType = 0) and over are not decoded and will generate 
     the above message in any case. Use the binary data elements in this 
     case.

