==================================================================
LX RemoteIO AX Wizard, Release 2.0.6 ReadMe File, September 17, 2010

Copyright (c) 2009 Johnson Controls Inc.      All Rights Reserved.
==================================================================

The Johnson Controls AX Wizards are client/server applications that 
require software to be installed on EC-BOS AX platforms and on any 
client machine running the Wizards.

This package contains software for the client machine to run the 
Johnson Controls RemoteIO Wizard.

After Setup the following versions will be installed on your computer:

- Johnson Controls RemoteIO Configuration 	Version 2.0
- ECC-301 External Interface File		LXIO301_v100.XIF
- ECC-301 Application Program       LXIO301_v115.APB
- ECC-301 Application Program       LXIO301_v115.NXE
- ECC-401 External Interface File		LXIO401_v100.XIF
- ECC-401 Application Program       LXIO401_v116.APB
- ECC-401 Application Program       LXIO401_v116.NXE
- ECC-520 External Interface File		LXIO520_v100.XIF
- ECC-520 Application Program       LXIO520_v115.APB
- ECC-520 Application Program       LXIO520_v115.NXE

I. Client installation (integrator computer)
============================================

This install procedure must be followed before using the RemoteIO 
AX Wizards. It is intended for any PC computer or laptop from which 
the RemoteIO AX Wizard will be configured.

Requirements : PC / Windows 2000, 2003, XP

1.  Run the setup "LX Remote IO Configuration v2.0.6 Setup"

II. Wizard initial running Instructions
=======================================

It is required to install the EC-NET-AX support pack 2.4.1 or 
later before using this Wizard.

The Wizard is launched from EC-NET-AX. See the instructions in the 
EC-NET-AX support package.

   
III. New Features and Problems fixed (Firmware)
====================================

Version 1.15 (LXIO301/LXIO520)and 1.16 (LXIO401) (16-09-2010)
	-	Bug fix: If to many inputs are configured in transtable, the device will loop in watchdog reset after a reset. Fixed


Version 1.14 (LXIO301/LXIO520)and 1.15 (LXIO401) (05-03-2008)
	- Modification : Improve detection of open circuit with PT100 and PT1000 thermistors.
	- Modification : Increase range limit from 135°C to 150°C for PT100 only.
	- Modification : Increase accuracy of PT100 and PT1000 sensors.
	- Modification : The calibration of PT100 and PT1000 sensors is now done in factory.
			 Only with UCPThardwareInfo.MajorVersion 2 and higher.

Version 1.01 (22-02-2007)

	- Bug fix : The controller needs to be reset to enable the input configuration changes. Fixed.
	- Bug fix : (For ECC-401 only) The inputs 9 to 12 were not reading properly. Fixed.

III. New Features and Problems fixed (Wizard)
====================================
	
version 2.0
	- initial release


IV. Known Problems and Workarounds
===================================

