==================================================================
LX-HPUL AX Wizard, Release 2.1.17 ReadMe File,    April 17, 2009

Copyright (c) 2009 Johnson Controls Inc.  All Rights Reserved.
==================================================================

The Johnson Controls AX Wizards are client/server applications that 
require software to be installed on EC-BOS AX platforms and on any 
client machine running the Wizards.

This package contains software for the client machine to run the 
Johnson Controls LX-HPUL Wizard.

This release is the initial release of the Johnson Controls 
LX-HPUL AX Wizard. After Setup the following versions will be 
installed on your computer:

- Johnson Controls LX-HPUL Configuration 	Version 2.1.17
- Johnson Controls Device Resource Files	Version 1.21			
- LX-HPUL External Interface File			    LXHPUL_v100.XIF
- LX-HPUL Application Program             LXHPUL_v114.APB
- LX-HPUL Application Program             LXHPUL_v114.NXE
- Sensor default ini file                 InputDefaultValues.ini

I. Client installation (integrator computer)
============================================

This install procedure must be followed before using the LX-HPUL 
AX Wizards. It is intended to any PC computer or laptop from which 
the LX-HPUL AX Wizard will be configured.

Requirements : PC / Windows 2000, 2003, XP

1.  Run the setup LX-HPUL Configuration v2.1.17 Setup.exe


II. Wizard initial running Instructions
=======================================

It is required to install the EC-NET-AX support pack 2.1.17 or 
later before using this Wizard.

The Wizard is launched from EC-NET-AX. See the instructions in the 
EC-NET-AX support package.

III.I New Features and Problems Fixed (Firmware)
====================================

Version 1.14

	- A new option was added to select the action of the reversing valve.
	- The reversing valve now turns off when all mechanical stages have been off for the
	  mechanical minimum off time.
	- It is now possible to short a transtable input to send the node in bypass mode.
	- Bug fix: The cooling stages were not disabled below minimum outdoor temperature. Fixed.

Version 1.04

	- Bug fix: The device is not able to switch to heating mode when a reversing valve output and
	  a fan state input are configured. Fixed.

Version 1.03

	- The apb is now compatible with the new plastic enclosure controller.
	- Bug fix: In some cases, the optimum start can leave the occupancy state in 
	  unoccupied mode during occupied or standby modes until the occupancy state is 
	  changed. Fixed.
	- Bug fix: When the REVERSING_VALVE is configured and the change over time is null or
	  the defrost cycle is activated, if the unit switches from cooling to heating, the 
	  reversing valve will stay OFF and the cooling will stay ON while there is a heating 
	  demand. Fixed.
	- Adjusted type 2 and 3 thermistor range (-40 to 150°C).

Version 1.02

	- Bug fix: When the REVERSING_VALVE is configured and the change over time is lower
	  than the cooling stage min ON time, the unit could switch from heating to cooling
	  without turning the reversing valve OFF thus staying always ON and heating while 
	  there is a cooling demand. Fixed.
	- Bug fix: After an optimum start has taken effect and the occupancy state is set to 
	  occupied, the unit status will display the morning warmup mode until a heating or 
	  cooling demand takes place. This bug has no internal effects. Fixed.

Version 1.01

	- Hardware outputs (analog) can now be configured as 2V to 10V.
	   
III.II New Features and Problems fixed (Wizard)
====================================

Version 2.1.17
	- The DRF files are updated to version 1.21.
	- The APB/NXE files are updated to version 114.
	- Changed: Removed "Emergency Contact Input Action"
	- Added: feature "Reversing normally heat and cool"
	- Fixed: The application couldn't show up to front 
	- Fixed: Sometimes when an output was selected (digital for example), the output type in the popped-up 
          actuator configuration did not have right type (DIGITAL for above example) in the selection list.
        - Fixed: When a HEAT_VALVE_ON_OFF output was configured and replicated the button "Apply", the "Permit 
	  valve radiation heating" disabled.
	- Fixed: when a output type was changed (from digital to analog for example), after selected the 'Cancel" 
	  button in the poped-up actuator configuration, the window closed but another poped-up actuator configuration
	  appeared again and the new selected type was not canceled. 
	- Changed: Help file updated.

IV. Known Problems and Workarounds
===================================

There are no known problems at the time of release.
